This is the USB driver installer for CobraRTP with FTDI USB controller (old).

Requirements:

 -Windows 7, 8, 8.1, 10, 11 (x64 Only) 
 -Requires Net Framework 3.5

To install, run the Setup v3.0 USB Driver.exe file and follow the instructions.

If the installation is unsuccessful, use the drivers from the site of the USB controller supplier: https://www.ftdichip.com/Drivers/VCP.htm
or use the automatically installed drivers by changing the “Latency Timer (msec)” from 16 to 1 for COMs in Device manager (See manual for Honda Edition).
Read more in the manual: cobrartp.com/en/downloads


cobrartp.com/en 2018-2022
cobrartpteam@gmail.com